130000

**HYBRIMATIC FINO urinal**

Артикул: 130000

Технические характеристики

Wall-hung individual urinal with HYBRIMATIC hybrid rinsing system:

HYBRIMATIC system:

- Battery-operated by 123 6V Lithium batteries.

- Concealed fluid detector.

- Waste with membrane and no water level.

- Electronics integrated into the urinal.

- Micro-rinse for one second after each user in Eco programme (or after 3 seconds in comfort programme).

- High frequency mode: rinse takes place after the busy period.

- Hygienic duty flush for 7 seconds every 24 hours in Eco mode (or for 14 seconds every 12 hours in comfort mode): prevents bad smells and blockages in the pipework.

- Flow rate pre-set at 0.07 L/sec. at 3 bar, can be adjusted.

- Stopcock.

Wall-hung FINO rimless urinal:

- Bacteriostatic 304 stainless steel, polished satin finish.

- Stainless steel thickness: 1.2mm.

- Rear water inlet.

- Recessed horizontal waste outlet.

Provisional availability: 1st half 2020. Please contact the sales office to check availbility.