50509P2

**Straight stainless steel grab bar, bright, Ø 32mm, 900mm**

Артикул: 50509P2

Технические характеристики

Straight grab bar for people with reduced mobility.

Tube Ø 32mm, 900mm centres, 1.5mm thick.

For use as a handrail and grab or support bar for WCs, showers or baths.

Bacteriostatic 304 stainless steel tube.

UltraPolish bright polished stainless steel, uniform non-porous surface for easy maintenance and hygiene.

Plate welded to the tube by invisible safety bead weld (process exclusive to "ArN-Securit").

40mm gap between the bar and the wall: minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

Concealed fixings secured by a 3-hole plate, 304 stainless steel, Ø 72mm.

Fixing plates and cover plates in 304 stainless steel.

Supplied with stainless steel screws for concrete walls.

 Tested to over 250kg. Maximum recommended user weight: 170kg.

10-year warranty. CE marked.