5055P2

**Straight stainless steel grab bar, bright, Ø 25mm, 300mm**

Артикул: 5055P2

Технические характеристики

Straight grab bar for people with reduced mobility.

Tube Ø 25mm, 300mm centres, 1.2mm thick.

For use as a handrail and grab or support bar for WCs, showers or baths.

Bacteriostatic 304 stainless steel tube.

Stainless steel with UltraPolish bright polished finish, uniform non-porous surface for easy maintenance and hygiene.

Plate welded to the tube by invisible safety bead weld (process exclusive to "ArN-Securit").

40mm gap between the bar and the wall: minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

Concealed fixings secured to wall by a 3-hole plate, 304 stainless steel, Ø 72mm.

Fixing plates and cover plates in 304 stainless steel.

Supplied with stainless steel screws for concrete walls.

Tested to over 200kg. Maximum recommended user weight: 115kg.

10-year warranty. CE marked.