5070GP2

**L-shaped stainless steel grab bar, bright, H. 750mm**

Артикул: 5070GP2

Технические характеристики

L-shaped grab bar Ø 32mm, for PRM, left model.

 Helps the user stand and secures movement in the bath or shower. Can be used as a shower rail by adding a sliding shower head holder and/or soap dish.

 Dimensions: 750 x 450mm.

Tube thickness: 1.5mm.

 Bacteriostatic 304 stainless steel tube.

Stainless steel with UltraPolish bright polished finish, uniform non-porous surface for easy maintenance and hygiene.

. Plate welded to the tube by invisible safety bead weld (process exclusive to "ArN-Securit”).

 40mm gap between the bar and the wall: minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

 Fixings concealed by a 3-hole cover plate, 304 stainless steel, Ø 72mm.

 Supplied with stainless steel screws for concrete walls.

 Tested to over 200kg. Maximum recommended user weight 135kg.

Bar comes with 10 year warranty. CE marked.