DELABIE_C100M355070N

**L-shaped Nylon shower grab bar, white, anti-bacterial, H. 750mm**

Артикул: 5070N

Технические характеристики

L-shaped shower grab bar Ø 32mm, for PRM.

Helps the user stand and secures movement in the bath or shower. Can be used as a shower rail by adding a sliding shower head holder and/or soap dish.

Dimensions: 750 x 450mm.

Can be installed with the upright to the left or right side.

Suitable for intensive use in public places or the healthcare sector.

High strength polyamide (Nylon): with 2mm reinforced steel core treated against corrosion.

Uniform non-porous surface for easy maintenance and hygiene.

Good resistance to chemical products and cleaning. Anti-UV treatment.

Warm to the touch.

38mm gap between the bar and the wall: minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

Fixings concealed by a 6-hole cover plate, Ø 73mm.

Supplied with stainless steel screws for concrete walls.

Tested to over 200kg. Maximum recommended user weight 135kg.

10-year warranty. CE marked.