DELABIE_C100M355082W

**Angled stainless steel grab bar 135°, white, 400 x 400mm**

Артикул: 5082W

Технические характеристики

Angled grab bar 135° for people with reduced mobility, Ø 32mm.

For use as a handrail (horizontal part) or as a grab bar (135° part) for WCs, showers or baths.

Universal for either left or right side.

Dimensions: 400 x 400mm.

Bacteriostatic 304 stainless steel tube, white powder-coated.

Plate welded to the tube by invisible bead weld (process exclusive to ArN-Securit).

40mm gap between the bar and the wall: minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

3 fixing points prevent the hand from getting trapped and simplify installation.

Concealed fixings, secured to wall on a 3-hole, 304 stainless steel plate, Ø 72mm.

Supplied with stainless steel screws for concrete walls.

Tested to over 250kg. Maximum recommended user weight: 170kg.

10 year warranty. CE marked.