DELABIE_C100M35510160S

**Stainless steel drop-down rail, satin, L. 650mm**

Артикул: 510160S

Технические характеристики

Drop-down grab bar Ø 32mm, for PRM.

In the lowered position use as a grab bar, for standing up and assisting movement. For WCs or showers. Allows side access in the raised position.

Dimensions: 650 x 230 x 105mm.

Retained in upright position. Slowed down descent.

Bacteriostatic 304 stainless steel tube.

Stainless steel with UltraSatin polished satin finish, non-porous uniform surface for easy maintenance and hygiene.

Fixings secured to wall by a 4mm thick 304 stainless steel fixing plate, concealed by cover plate.

Supplied with stainless steel screws for concrete walls.

Tested to over 200kg. Maximum recommended user weight 135kg.

10-year warranty. CE marked.