510161S

**Fixed wall support bar Ø 32mm, L. 650mm**

Артикул: 510161S

Технические характеристики

Wall support bar for people with reduced mobility, Ø 32mm.

For use as a grab bar and a fixed support bar for WCs, showers or washbasins.

Generally installed parallel to a drop-down rail in a WC or on either side of a washbasin.

Recommended if the WC pan or shower seat is a long way from the side wall.

Dimensions: 650 x 230 x 105mm, Ø 32mm.

Bacteriostatic 304 stainless steel tube.

Stainless steel with UltraSatin polished satin stainless steel, uniform non-porous surface for easy maintenance and hygiene.

Fixings secured to wall by a 4mm thick 304 stainless steel fixing plate, concealed by cover plate.

Supplied with stainless steel screws for concrete walls.

Tested to over 200kg. Maximum recommended user weight 135kg.

 10-year warranty. CE marked.