510629S

**Comfort backrest for WCs**

Артикул: 510629S

Технические характеристики

Comfort backrest for WCs with structure in UltraSatin polished satin 304 stainless steel, for PRM.

Backrest made from soft polyurethane.

Tube Ø 25mm x 12mm.

Fixings concealed by a 3-hole cover plate, 304 stainless steel, Ø 72mm.

Dimensions: 150 x 580 x 173mm.

CE marked.