DELABIE_C100M355160N

**Drop-down rail, Ø 32mm, L. 650mm**

Артикул: 5160N

Технические характеристики

Drop-down grab bar Ø 32mm, for PRM. HR Nylon bright white.

In the lowered position use as a grab bar, as a support for standing up and for assisting movement, for WCs or showers. Allows side access in the raised position.

Dimensions: 650 x 230 x 105mm

Slowed descent. Retained in upright position.

Suitable for intensive use in public places or the healthcare sector.

High-strength polyamide (Nylon) and polymer: with 2mm reinforced steel core treated against corrosion.

Uniform non-porous surface for easy maintenance and hygiene.

Good resistance to chemical products and cleaning. Anti-UV treatment.

Warm to the touch.

Fixings, secured to wall by a 4mm thick 304 stainless steel plate, concealed by cover plate.

3 fixing points allow the stop of the wrist and an easy installation.

Supplied with stainless steel screws for concrete walls.

Tested to over 200kg. Maximum recommended user weight 135kg.

10-year warranty. CE marked.