5440N

**T-shaped white anti-bacterial Nylon grab bar**

Артикул: 5440N

Технические характеристики

T-shaped shower grab bar, Ø 32mm, for preople with reduced mobility.

 Use as a support rail and to support the user in an upright position. Helps and secures entry and movement in the shower. Use as a shower rail by adding a sliding shower head holder

and/or soap dish.

 Anti-bacterial NylonClean treatment: increased protection against bacterial development.

 Can support a removable shower seat (order separately).

 Dimensions: 1,150 x 500mm.

 Suitable for intensive use in public places or the healthcare sector.

 High strength polyamide (Nylon):

with 2mm reinforced steel core treated against corrosion.

 Uniform non-porous surface for easy maintenance and hygiene.

 Good resistance to chemical products and cleaning. Anti-UV treatment.

 Warm to the touch.

 38mm gap between the bar and the wall: minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

 Fixings concealed by a 6-hole cover plate, Ø 73mm.

 Supplied with stainless steel screws for concrete walls.

Dimensions: 1,150 x 500mm.

 Tested to over 200kg. Maximum recommended user weight: 135kg.

10-year warranty. CE marked.