5440P2

**T-shaped polished stainless steel shower grab bar**

Артикул: 5440P2

Технические характеристики

T-shaped shower grab bar, Ø 32mm, for preople with reduced mobility.

Use as a support rail and to support the user in an upright position.

 Assists entry and movement in the shower. Use as a shower rail by adding a sliding shower head holder and/or soap dish.

 Chrome-plated sliding shower head holder with ergonomic locking ring.

 Possible to add a sliding soap dish (order separately).

 Dimensions: 1,150 x 500mm.

 Bacteriostatic 304 stainless steel tube.

 Stainless steel with UltraPolish bright, non-porous uniform surface for easy maintenance and hygiene.

 Plate welded to the tube by invisible bead weld (process exclusive to ArN-Securit).

40mm gap between the bar and the wall: minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

Concealed fixings, secured to wall by a 3-hole plate Ø 72mm.

 304 stainless steel plates and covers.

 Supplied with stainless steel screws for concrete walls.

 Tested to over 200kg. Maximum recommended user weight 135kg .

10-year warranty. CE marked.