5490N

**Two-wall corner shower grab bar with vertical bar Ø 32mm**

Артикул: 5490N

Технические характеристики

Two wall corner shower grab bar with vertical bar, for people with reduced mobility, Ø 32mm.

Can be used as a support rail and to support the user in an upright position. Helps and secures entry and movement in the shower.

Can be used as a shower rail by adding a sliding shower head holder and/or soap dish.

Can support a removable shower seat (order separately).

Dimensions: 1,150 x 750 x 750mm.

Can be installed with the upright to the left or right side.

Suitable for intensive use in public places or the healthcare sector.

High strength polyamide (Nylon): with 2mm reinforced steel core treated against corrosion.

Uniform non-porous surface for easy maintenance and hygiene.

Good resistance to chemical products and cleaning. Anti-UV treatment.

Warm to the touch.

38mm gap between the bar and the wall: minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

Fixings concealed by a 6-hole cover plate, Ø 73mm.

Supplied with stainless steel screws for concrete walls.

Tested to over 200kg. Maximum recommended user weight 135kg.

10-year warranty. CE marked.