792400

**SECURITHERM shower panel**

Артикул: 792400

Технические характеристики

Thermostatic electronic shower panel:

 Anodised aluminium shower panel for wall-mounted, exposed installation.

With top inlet, via in-line stopcocks M1/2".

 SECURITHERM thermostatic mixer.

Adjustable temperature control from cold water up to 38°C with 1st limiter set at 38°C and 2nd limiter set at 41°C.

Anti-scalding safety: automatic shut-off if cold or hot water supply fails.

 Thermal shocks are possible.

 Battery-operated with 223 6V Lithium battery.

Infrared presence detection. Shower starts when hand is 4cm from the sensor.

 Shuts off on demand or automatically after ~60 seconds.

 Duty flush (~60sec. every 24hr after the last use).

 Flow rate set at 6 lpm at 3 bar.

Chrome-plated, tamperproof, scale-resistant ROUND shower head with automatic flow rate regulation.

 Concealed fixings.

Filters and non-return valves.

10-year warranty.