DELABIE_C100M35H9769

**SECURITHERM Securitouch thermostatic shower mixer**

Артикул: H9769

Технические характеристики

SECURITHERM dual control thermostatic shower mixer with:

- No non-return valves on the inlets (reduced bacterial proliferation).

No risk of cross flow between hot and cold water.

- Anti-scalding failsafe: shuts off immediately if cold water supply fails (and vice versa).

- Securitouch thermal insulation prevents burns.

- Scale-resistant thermostatic cartridge for temperature adjustment.

- ¼-turn ceramic head for flow rate adjustment.

- Temperature control up to 41°C.

- Double temperature limiter: 1st limiter set at 39°C, 2nd limiter set at 41°C.

- Thermal shocks are possible with removing the control knob or shutting off the cold water supply.

- Flow rate limited to 9 lpm.

- Ergonomic controls.

- M½" shower outlet.

- M¾" inlets with integrated filters.

Mixer supplied with STOP/CHECK wall connectors M½" M¾", ideal for hospitals.

10-year warranty.