510629N

**Comfort backrest for WCs**

Артикул: 510629N

Технические характеристики

Comfort backrest for WCs with white, high strength polyamide (Nylon) structure, for PRM.

Backrest made from soft polyurethane.

Tube Ø 32mm.

Fixings concealed by a 6-hole cover plate, Ø 73mm.

Dimensions: 150 x 575 x 173mm.

CE marked.