5630

**Single hole pre-rinse set**

Артикул: 5630

Технические характеристики

Complete pre-rinse set without bib tap.

Deck-mounted single hole mixer with:

- Valve heads with reinforced mechanisms and ergonomic control levers.

- F3/8" flexibles and non-return valves.

- Reinforced fixing via 2 threaded rods with back-nuts.

Black, scale-resistant M1/2" hand spray with adjustable jet and 9 lpm flow rate at the outlet.

Black, reinforced, food-grade flexible hose L. 0.95m.

3/4" brass column.

Adjustable wall bracket.

Stainless steel spring guide.

10-year warranty.